<?xml version="1.0" encoding="UTF-8" standalone="yes"?>
<!--AMCI Stop Jog-->
<RSLogix5000Content SchemaRevision="1.0" SoftwareRevision="20.05" TargetName="AMCI_NXFE2_Stop_Jog" TargetType="AddOnInstructionDefinition" TargetRevision="1.0 " TargetLastEdited="2025-12-19T20:05:45.356Z" ContainsContext="true" Owner="root" ExportDate="Fri Jan 02 09:35:31 2026" ExportOptions="References DecoratedData Context Dependencies ForceProtectedEncoding AllProjDocTrans">
<Controller Use="Context" Name="NXFE2_EDS_AOI_sample_RSLogix_V20">
<DataTypes Use="Context">
<DataType Name="AMCI_NXFE2_Output_Data" Family="NoFamily" Class="User">
<Members>
<Member Name="Command_Word_0" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Command_Word_1" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Position_or_Distance" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Programmed_Speed" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Acceleration" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Deceleration" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Reserved_Word_8" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Reserved_Word_9" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
</DataType>
<DataType Name="AMCI_NXFE2_Input_Data" Family="NoFamily" Class="User">
<Members>
<Member Name="ZZZZZZZZZZAMCI_NXFE20" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="MovingCW" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="0" ExternalAccess="Read/Write"/>
<Member Name="MovingCCW" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="1" ExternalAccess="Read/Write"/>
<Member Name="InHoldState" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="2" ExternalAccess="Read/Write"/>
<Member Name="Stopped" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="3" ExternalAccess="Read/Write"/>
<Member Name="AtHome" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="4" ExternalAccess="Read/Write"/>
<Member Name="Accelerating" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="5" ExternalAccess="Read/Write"/>
<Member Name="Decelerating" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="6" ExternalAccess="Read/Write"/>
<Member Name="MoveComplete" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE20" BitNumber="7" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZAMCI_NXFE29" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="HomeInvalid" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="0" ExternalAccess="Read/Write"/>
<Member Name="ProfileInvalid" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="1" ExternalAccess="Read/Write"/>
<Member Name="PositionInvalid" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="2" ExternalAccess="Read/Write"/>
<Member Name="InputError" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="3" ExternalAccess="Read/Write"/>
<Member Name="CommandError" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="4" ExternalAccess="Read/Write"/>
<Member Name="ConfigurationError" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="5" ExternalAccess="Read/Write"/>
<Member Name="ModuleOK" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="6" ExternalAccess="Read/Write"/>
<Member Name="ModeFlag" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE29" BitNumber="7" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZAMCI_NXFE218" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="CaptureInputActive" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="0" ExternalAccess="Read/Write"/>
<Member Name="ExternalInputActive" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="1" ExternalAccess="Read/Write"/>
<Member Name="HomeInputActive" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="2" ExternalAccess="Read/Write"/>
<Member Name="CWLimitActive" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="3" ExternalAccess="Read/Write"/>
<Member Name="CCWLimiitActive" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="4" ExternalAccess="Read/Write"/>
<Member Name="NoFaultOutputState" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="5" ExternalAccess="Read/Write"/>
<Member Name="OnLineOutputState" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="6" ExternalAccess="Read/Write"/>
<Member Name="MoveCompleteOutputState" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE218" BitNumber="7" ExternalAccess="Read/Write"/>
<Member Name="ZZZZZZZZZZAMCI_NXFE227" DataType="SINT" Dimension="0" Radix="Decimal" Hidden="true" ExternalAccess="Read/Write"/>
<Member Name="RunningBlendMove" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="0" ExternalAccess="Read/Write"/>
<Member Name="BlendMoveACK" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="1" ExternalAccess="Read/Write"/>
<Member Name="NonZeroMinRegDistance" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="2" ExternalAccess="Read/Write"/>
<Member Name="Reserved_bit_11" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="3" ExternalAccess="Read/Write"/>
<Member Name="BckplnHomeProxBitState" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="4" ExternalAccess="Read/Write"/>
<Member Name="EncoderFollowerMode" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="5" ExternalAccess="Read/Write"/>
<Member Name="Reserved_bit_14" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="6" ExternalAccess="Read/Write"/>
<Member Name="Reserved_bit_15" DataType="BIT" Dimension="0" Radix="Decimal" Hidden="false" Target="ZZZZZZZZZZAMCI_NXFE227" BitNumber="7" ExternalAccess="Read/Write"/>
<Member Name="MotorPosition" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="EncoderPosition" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="CaptureData" DataType="DINT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="Reserved_Word_8" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
<Member Name="NetworkConnectivity" DataType="INT" Dimension="0" Radix="Decimal" Hidden="false" ExternalAccess="Read/Write"/>
</Members>
</DataType>
</DataTypes>
<AddOnInstructionDefinitions Use="Context">
<AddOnInstructionDefinition Use="Target" Name="AMCI_NXFE2_Stop_Jog" Revision="1.0" Vendor="AMCI" ExecutePrescan="false" ExecutePostscan="false" ExecuteEnableInFalse="true" CreatedDate="2011-05-06T14:19:37.914Z" CreatedBy="AMCI_HQ\jsutula" EditedDate="2025-12-19T20:05:45.356Z" EditedBy="AMCI-MC\jsutula"
 SoftwareRevision="v20.05">
<Description>
<![CDATA[AMCI Stop Jog]]>
</Description>
<RevisionNote>
<![CDATA[12/19/2025 Initial Release]]>
</RevisionNote>
<AdditionalHelpText>
<![CDATA[AXIS INPUT DATA:  Input data from the NXFE2.   Uses the AMCI_NXFE2_Input_Data User Defined Data Type.  

AXIS OUTPUT DATA; Output data from the AOI to the AMCI NXFE2.    Uses the AMCI_NXFE2_Output_Data User Defined Data Type.  


EN (Enable) Set when rung is true, Reset when rung is false
DN (Done) Set when command is sent to the motion device.  Reset when the rung is false.   
ER (Error) Set when there is a command or input error.  Reset when the rung is false.   ]]>
</AdditionalHelpText>
<Parameters>
<Parameter Name="EnableIn" TagType="Base" DataType="BOOL" Usage="Input" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Input - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="EnableOut" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="false" ExternalAccess="Read Only">
<Description>
<![CDATA[Enable Output - System Defined Parameter]]>
</Description>
</Parameter>
<Parameter Name="NXFE2_Input_Data" TagType="Base" DataType="AMCI_NXFE2_Input_Data" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="NXFE2_Output_Data" TagType="Base" DataType="AMCI_NXFE2_Output_Data" Usage="InOut" Required="true" Visible="true" Constant="false"/>
<Parameter Name="EN" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read/Write">
<Description>
<![CDATA[set when rung with AOI is true]]>
</Description>
<DefaultData>00</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="DN" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[set when reset error command sent to motion axis]]>
</Description>
<DefaultData>00</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
<Parameter Name="ER" TagType="Base" DataType="BOOL" Usage="Output" Radix="Decimal" Required="false" Visible="true" ExternalAccess="Read Only">
<Description>
<![CDATA[set when reset error command did not clear the error]]>
</Description>
<DefaultData>00</DefaultData>
<DefaultData Format="Decorated">
<DataValue DataType="BOOL" Radix="Decimal" Value="0"/>
</DefaultData>
</Parameter>
</Parameters>
<LocalTags>
<LocalTag Name="command_data_block" DataType="INT" Dimensions="10" Radix="Decimal" ExternalAccess="Read/Write">
<DefaultData>00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 
00 00 00 00</DefaultData>
<Comments>
<Comment Operand="[0]">
<![CDATA[Command Bits MSW]]>
</Comment>
<Comment Operand="[1]">
<![CDATA[Command Bits LSW]]>
</Comment>
<Comment Operand="[2]">
<![CDATA[Upper Target Position]]>
</Comment>
<Comment Operand="[3]">
<![CDATA[Lower Target Position]]>
</Comment>
<Comment Operand="[4]">
<![CDATA[Upper Programmed Speed]]>
</Comment>
</Comments>
<DefaultData Format="Decorated">
<Array DataType="INT" Dimensions="10" Radix="Decimal">
<Element Index="[0]" Value="0"/>
<Element Index="[1]" Value="0"/>
<Element Index="[2]" Value="0"/>
<Element Index="[3]" Value="0"/>
<Element Index="[4]" Value="0"/>
<Element Index="[5]" Value="0"/>
<Element Index="[6]" Value="0"/>
<Element Index="[7]" Value="0"/>
<Element Index="[8]" Value="0"/>
<Element Index="[9]" Value="0"/>
</Array>
</DefaultData>
</LocalTag>
</LocalTags>
<Routines>
<Routine Name="EnableInFalse" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[XIC(EN)MOV(0,command_data_block[0])MOV(command_data_block[0],NXFE2_Output_Data.Command_Word_0);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[OTU(EN)OTU(DN)OTU(ER);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
<Routine Name="Logic" Type="RLL">
<RLLContent>
<Rung Number="0" Type="N">
<Text>
<![CDATA[OTL(EN);]]>
</Text>
</Rung>
<Rung Number="1" Type="N">
<Text>
<![CDATA[[XIC(NXFE2_Input_Data.InputError) ,XIC(NXFE2_Input_Data.CommandError) ]MOV(0,command_data_block[0])OTE(ER);]]>
</Text>
</Rung>
<Rung Number="2" Type="N">
<Comment>
<![CDATA[The following rung moves a decimal value of "0" into the command word.  This command will stop a running jog using the deceleration rate of the jog command.              ]]>
</Comment>
<Text>
<![CDATA[MOV(0,command_data_block[0])OTL(DN);]]>
</Text>
</Rung>
<Rung Number="3" Type="N">
<Comment>
<![CDATA[Move the command block data internal to the Add on Instruction to the output registers assigned to the AMCI NXFE2.  ]]>
</Comment>
<Text>
<![CDATA[MOV(command_data_block[0],NXFE2_Output_Data.Command_Word_0);]]>
</Text>
</Rung>
</RLLContent>
</Routine>
</Routines>
<Dependencies>
<Dependency Type="DataType" Name="AMCI_NXFE2_Input_Data"/>
<Dependency Type="DataType" Name="AMCI_NXFE2_Output_Data"/>
</Dependencies>
</AddOnInstructionDefinition>
</AddOnInstructionDefinitions>
</Controller>
</RSLogix5000Content>
